{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["参数调研清单"],"not_rendered":{"defined_names":1},"read":"whole","date_system":"1900"}

{"sheet":"参数调研清单","index":0,"n_rows":31,"n_cols":5,"rows_kept":31,"merged":[[0,0,0,4],[1,0,15,0],[16,0,23,0],[24,0,29,0],[30,0,37,0],[30,1,37,4]]}
["低温甲醛蒸汽灭菌器维护保养服务参数调研清单"]
["功能性参数","序号","详细项目","产品是否符合（是/否）","备注(若不符合请在此栏填写所提供产品相应功能)"]
[null,1,"▲维保设备：2台低温蒸汽甲醛灭菌器(型号130LF），序列号为E-28335和E-29892，以及设备配套的2台水冷机（型号BS-03WS）。"]
[null,2,"服务响应时间：服务响应时间为0.5小时内，工程师到位时间4小时(本市)。"]
[null,3,"维修时间：现场工程师根据设备情况采取必要的临时性保障措施，在确保各项安全的前提下，快速恢复设备的运行；当遇到较大设备故障时，应及时的给出解决方案，及各项准备工作，并于48小时内完成设备维修。"]
[null,4,"维保产品须符合中华人民共和国强制性技术标准。"]
[null,5,"设备巡检服务：维保年度内，每年提供至少四次巡检服务。"]
[null,6,"设备维护保养服务：维保年度内，每年进行一次设备维护保养作业。"]
[null,7,"服务期内，包含不限次数的人工服务，不另外收费。"]
[null,8,"服务期内，维修及零配件不另外收费。"]
[null,9,"维修及保养记录：保修期内，每次故障维修及保养，提供维修及保养记录并到医疗设备科备案。"]
[null,10,"保证备件的存储，并提供备件的优先发货。"]
[null,11,"因维护保养不当，造成的相关损失，由维保供应方承担相应的责任。"]
[null,12,"▲保障设备开机率要达到95%，每年不超过18天（365天计），超过1天保修期顺延1天。凡不在维修范围内的设备停机，不包括在此条款内。"]
[null,13,"维保供应方应根据科室需要提供与消毒灭菌设备相关的附属设备的技术支持服务与培训服务。"]
[null,14,"▲维保年限：3年。"]
["配置需求","序号","详细项目","配置数量","备注(可根据实际产品自行补充)"]
{"$rows_empty":7}
["补充参数\n\n（根据产品本身可自行补充，若无，可不填写）","序号","详细项目","产品参数","备注"]
[]
[]
[]
[]
[]
["针对本项目采购需求内容的优化建议"]